Cruise/Data Start Date in GMT=10/23/2008-22:44:59
Cruise/Data Stop Date in GMT=10/26/2008-00:42:26
Cruise Distance=389.843
NOTES=Sample 9 taken @ #### m deep, ####m total depth, Sta 307, Cast 256
YOUNG-TWIND Direction/ Speed=This is the calculated true wind direction/Spd using ship spd/heading and realtive wind spd/dir
LOW Sea Temp=This is a seawater temp sensor located approx 2m below the surface, in Deg C
Met Sensors=These datas are provided by a Young  Met consol. Temps are in Deg C and Baro Press is in hPa
EK 60 depth=This is the depth below the SURFACE and is adjusted for water temp/Sound Spd/Salinity and TX depth.
GYRO=The GYRO is the Ship's navigational gyrocompass giving the direction magnetic true that the ship is pointing
MX420 =The MX420 is the Ship's GPS givng Speed over ground SOG, Course over Ground COG and Lal/Lon
CTD=CTD, SBE 19+ s/n 4759, data will only appear during a CTD cast.
TSG and Flowmeter-ma=SBE 45 micro TSG s/n 0177, may be intermitten due to pump's operational constraints. When Flow rate is zero data should be disregarded. Flow rate in gal/min
